**Scrubber Basic Functions**

* Dispenses & meters solution
* Scrubs floors (and captures light debris if cylindrical)
* Recovers used solution
* Leaves floors Clean, Safe and Dry

**Stage 1 – Establish Your Value**

* You
* Your Dealer
* Advance

**For Stages 2 – 4 Just Follow the Solution Flow**

**Stage 2 – Solution System**

* Large 37 gallon (140 liter) capacity
* EcoFlex™ system (optional)
* Solution level integrated with brush pressure selection
* SmartFlow™ – solution control
* Externally removable filter/screen

**Stage 3 – Scrub System**

* 34” disc, 32” and 36” cylindrical
* Offset deck for edge cleaning
* Self-adjusting side skirts provide excellent water containment
* Three down pressure settings with scrub pressure up to 230 lb (disc)
* Powerful 1hp x 2 scrub motors for disc and .74 hp x 2 for cylindrical decks
* Ruggedized cylindrical drive system for 4x reliability increase
* Auto click-on disc brush system
* No tools, cylindrical brush access
* Optional side broom for 32” cylindrical

**Stage 4 – Recovery System**

* Pivoting squeegee with Linatex™ blades
* Vac hose stays connected to connection flange when installing squeegee
* Powerful vac system (dual vac optional)
* Large vacuum recovery hose to minimize plugging
* Debris catch tray
* Industrial strength full tank float switch
* Pinch flow control drain hose

**Stage 5 – Power Systems and Service**

* MaxAccess™ design
* Yellow knobs as service points
* Sturdy, tubular steel frame
* Front tubular steel bumper (optional)
* Rotomold, corrosion free durability
* SST fasteners (or plated) for wetted machine components
* Variable speed, AC brushless drive
* Over 6 hours run time with 420 AH, C20 battery (in typical applications)
* Tools-free for routine maintenance
* Embedded electronic diagnostics

**Stage 6 – Operator Interface**

* Clear-View™ operator compartment
* Ergonomic design with tilt steering
* One Touch controls w/integrated brush pressure and solution flow rate
* SmartKey multi-user control w/impact detection
* Single pedal for forward/reverse motion control
* 63” (160 cm) minimum aisle U-turn
* Bright, clear OLED display providing information at your fingertips
* Fingertip paddle controls for horn, Burst of Power, & intermittent solution off
* Scrub speed limiter feature
* Menu for organized information on service and machine configuration

**Extras - Options**

* Side broom for 32” cylindrical (right side)
* Heavy duty tubular front metal bumper
* Off aisle vac wand
* Blue safety warning light
* Overhead guard with Clear-View design
* Dual LED front headlights
* Warning beacon
* Deluxe suspension seat
* Dual recovery vac
* Solution auto-fill
* Squeegee guard
* EcoFlex
* Foot Guard
* USB charging port w/phone holder